**Scope of Work:**

Vendor shall furnish all labor, materials, tools, equipment, and supplies necessary to remove the existing rolling doors and install new doors at the Louisiana State Penitentiary (LSP).

**Jobsite Location:**

Louisiana State Penitentiary

17544 Tunica Trace (Hwy 66)

915 Warehouse

Angola, LA 70712

**Jobsite Visit Contact:**

Danielle Matherne

danielle.matherne@la.gov

225-655-2589

**Job Specifications:**

Vendor shall remove two (2) existing odd sized rolling steel doors that were retrofitted to the main metal building frame structure. Vendor shall then re-frame using structural steel on the sides and eight inch (8") metal across the top, so that new standard size ten foot by ten foot (10' x 10') doors can be installed using the new framework.

After new frame is constructed, vendor shall furnish and install two (2) new sheet doors with chain hoist. New installed rolling doors shall be manually operated.

**Door Specifications:**

\* Ten foot by Ten foot (10' x 10')

\* Twenty six (26) gauge galvanized steel curtain, eighty thousand (80,000) psi

\* Roll-formed steel sections, interlocked and seamed to form full door

\* Flexible webbing on both front edges

\* Counterbalance assembly: twelve inch (12") steel stepped rings

\* Universal guides: eighteen (18) gauge roll-formed galvanized steel with pre punched through hole design

\* Head plate: eleven (11) gauge steel

\* Bottom bar: extruded aluminum reinforced with steel, roll-formed angles

\* Quick connect bottom bar stops- twelve (12) gauge galvanized steel

\* Bottom seal: bulb type, extruded aluminum reinforced with roll formed steel angle

\* Guide rub strips: three inch (3") wide polypropylene strips on both edges

\* Standard springs: three and three eighths inch (3-3/8") torsion springs

\* Locks shall be slide bolt type mounted on each end of the doors bottom bar assembly by locking into the door guide, eleven (11) gauge steel

\* Color: white

ProStar model # 780CD or equal

**Specify Brand/Model of Rolling Door Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**General Terms and Conditions:**

\* All work being performed is required during normal business hours within secure care facilities.  Monday through Friday 7:00 A.M. to 3:30 P.M.

\* Work to be performed in a workmanlike manner according to standard, and meet all code requirements, federal, state and local.

\* All equipment shall have a minimum one (1) year manufacturer’s warranty. Workmanship shall be covered by a one (1) year warranty for all installation work.

\* Vendor representatives are subject to passing a background check.

\* Vendors are subject to vehicle searches.

\* Vendor representatives must follow all policy and procedures while performing work on facility grounds.