Removal and Replacement of Refrigerant Monitor

**Location:**

Central Louisiana Supports and Services Center

5400 Coliseum Boulevard

Alexandria, LA 71303

**Scope of work:**

Contractor shall provide all labor, materials, tool, and equipment necessary to remove existing refrigerant monitor and replace with a new Trane RMWE refrigerant monitor, or equal.

**Requirements:**

* Contractor shall disconnect the main power supplying defective refrigerant monitor, as well as disconnect the refrigerant monitor from the strobe lights and exhaust fan.
* Contractor shall and remove from service and dispose of existing refrigerant monitor.
* Contractor shall install new Trane RMWE refrigerant monitor, or equal to, that has four (4) sample ports for R-134a refrigerant.
  + If not bidding as specification, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* Contractor shall connect new refrigerant monitor to strobe lights and exhaust fans .
* Contractor shall also test the operation on the refrigerant monitor after the installation has been completed. Contractor shall have the Facility Manager present for testing.

**Other Requirements:**

* Contractor shall be responsible for removal and cleanup of all debris resulting from work performed.
* Contractor shall provide the Manufacturer’s warranty.