**Scope of Work:**

Contractor shall provide all labor and materials (except for existing card readers that are to be moved) in order to install four automatic door openers, move four card readers, and install one card reader and lock set for the Louisiana Department of Health (LDH). Contractor shall be responsible for cleanup of any debris.

**Location:**

Central Louisiana Supports and Services Center

5400 Coliseum Boulevard

Alexandria, LA 71303

**Contact:**

Darrell Carson, Facility Maintenance Manager A

318-542-9002

**Specifications:**

-Contractor shall install four LCN 9540 (or equivalent) reverse electromechanical door openers.

**Specify Brand/Model of door opener bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

-Two shall be installed on building #20 Transitional Family Life Center; one at the front entrance and one at the back exit door.

-One shall be installed on building #21 Transition building entrance door.

-One shall be installed on building #6 Cafeteria door facing the playground.

-Contractor shall move existing card readers for residents to be able to access.

-Two card readers are to be moved on building #20 Transitional Family Life Center at the front entrance and the back exit door.

-One card reader relocated on building #21 Transition building entrance door.

-One care reader relocated on building #6 Cafeteria door facing the playground.

**\*The expansion chassis has been approved as a proprietary purchase and only the brand/model specified will be considered for award.**

-Contractor shall install one Brivo ACS6100 regular expansion chassis (current system is a Brivo) in the nurse’s station in building #20 Transitional Family Life Center.

-Expansion chassis system shall include the following components:

Install one regular enclosure with lock

Install one B-ACS6100-PSB internal power supply board

Install one Plug-in AC/C power adapter

Install one 12v 14Ah sealed lead acid battery backup

Install one Single gang tri-technology reader with keypad (black enclosure)

Install one Two-reader expansion board with OSDP

-Contractor shall install one modular Strike for Mortise and cylindrical lockset, stainless steel, satin, field selectable voltage 12 or 24vdc and 12 volt to 24VAC.

-Contractor shall run compatible wire from Transitional Family Life Center building #20 to Transitional gym building #21 in order for nurse’s station card reader to work.

-Contractor shall perform a system test to make sure all equipment is functioning properly.