**Scope of Work:**

Contractor shall provide labor, material, tools, and equipment necessary to establish grade and install a concrete drainage system to drain water from back parking area to the north side of the sally port road and remove existing asphalt and lay approximately 4,700 square feet of asphalt in the sally port/fuel bay area. New asphalt shall be extended to existing asphalt. Contractor shall also haul and dispose waste materials off-site at an EPA approved site of Contractor’s choice.

**Location:**

David Wade Correctional Center

670 Bell Hill Road

Homer, LA 71040

**Requirements:**

* Contractor shall establish grade and install a concrete formed steel drain with footers and heavy industrial grade metal grating. Approximately 24 yards of concrete.
	+ Grade shall be 22 feet in length by 12 feet in width.
	+ Drain shall be 22 feet in length by 12 inches in width.
* Contractor shall tear out existing asphalt and lay new asphalt. Approximately 4,700 square feet of road with asphalt.
	+ Contractor shall tear out existing asphalt 3 inches in depth and haul off site.
	+ Contractor shall lay new asphalt 3 inches in depth where existing asphalt was.
	+ Contractor shall lay new asphalt 3 inches in depth to widen the sally port road turning area.
* Existing road is approximately 20 feet wide.
* See Attachment D – Maps for locations of the areas.
* All work shall be performed between the hours of 8:00 am to 3:30 pm (central time) Monday-Friday.
* No firearms, knives, drugs, cell phones, etc., are allowed within facility. Vehicles shall be searched upon entry and departure. Identification is required to enter facility.

Contact Pat Blackwelder DWCC maintenance supervisor for site visit and job questions. E-mail: Patrick.blackwelder@la.gov Phone: 318-927-0400 ask for Pat Blackwelder in maintenance.