Attachment C – Line Item Responses

RFx No.: 3000022830 \*Site Visit\*Fax\* Building Materials-LDWF

\*Complete the table with the information you are bidding.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **DESCRIPTION** | **QTY** | **# PIECES** | **LENGTH** | **TYPE/COLOR** | **DIMENSIONS** |
| 1 | 5 Hole anchor plate |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 2 | Tubing 4X4 11 GA |  |  |  |  |  |
| 3 | 36’ 2/12 End, 6” Rake |  |  |  |  |  |
| 4 | 36’ 2/12 Middle, 6 |  |  |  |  |  |
| 5 | Eve Strut 14GA 6X4X20 |  |  |  |  |  |
| 6 | Cee Purlin 6X2X20’ |  |  |  |  |  |
| 7 | Cee Purlin 4X2X20’ |  |  |  |  |  |
| 8 | Channel 30’ 14GA 4 3/16X2 |  |  |  |  |  |
| 9 | Tubing 4X4X30’ 14Ga (Red) |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 10 | AKZO 1050CC 26G Emerald Green |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 11 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
| 12 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
| 13 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
| 14 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
| 15 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
| 16 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
| 17 | AKZO 1050CC 26G Lightstone |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 18 | 16’ Industrial Outside Corner Color |  |  |  |  |  |
| 19 | 16’ Industrial Head Trim Color |  |  |  |  |  |
| 20 | 10’ Industrial Head Trim Color |  |  |  |  |  |
| 21 | 10’ Post Patio Eave 6.5” Color |  |  |  |  |  |
| 22 | 20” Post Patio Rake 7.25” Color |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 23 | 10’ Residential Ridgecap 20” Color |  |  |  |  |  |
| 24 | pdf (post drip flashing)  3”back Special Trim |  |  |  |  |  |
| 25 | 10’ Mini Jamb Cover Color |  |  |  |  |  |
| 26 | 16’ Mini Jamb Cover Color |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 27 | Emerald Green Laptek Screw 7/8 |  |  |  |  |  |
| 28 | Lightstone Tek Screws 1” |  |  |  |  |  |
| 29 | Emerald Green Tek Screws 1” |  |  |  |  |  |
| 30 | Sealant 3/8 x 3/32 x 45 Ft Roll Gray |  |  |  |  |  |
|  |  |  |  |  |  |  |
| 31 | 3068 Walk Door (AS3) |  |  |  |  |  |