**Tractor Truck Specifications**

NOTE: This item has been approved as a proprietary purchase and only the make and model specified will be considered.

**Peterbilt Model 579 Tractors with 44-inch Low Roof Sleeper, Clone of Chassis 747906 Model 579**

* **Rear Mudflaps and Coil Hangers**
* **Polyarmor Black Quarter Fenders**
* **JOST JSK36 Fifth Wheel, Light Weight Top Plate**
* **7.6in – 8-in Fifth Wheel Height with 18" Air Slide**
* **Frame Mounted Deckplate and Access Pkg, RH Side**
* **PHP10 Iron Preset PLUS Hubs - Front and Rear**
* **Bendix Air Cam Front HP Drum Brakes 16.5x5**
* **Gusseted Cam Brackets, Steer Axle - Front and Rear**
* **Heavy Duty Cam Bushings, Steer Axle - Front and Rear**
* **Anti-Lock Braking System (ABS) 6S6M**
* **Omit SmarTire Tire Pressure Monitoring**
* **Bendix Air Cam Rear Drum Brakes 16.5x7 with Automatic Slack Adjusters & Outboard Mounted Brake Drums.**
* **Ratio 3.36 Rear Axle**
* **Peterbilt Low Low Air Leaf 40,000 lb, 52-in Axle Spacing, Light Weight.**
* **Dash mounted dump switch with indicator light for suspension.**
* **PACCAR MX-13 455 @1600 GV@2200 1650@900 (2024 Emissions)**
* **Enable Preferred EIST Settings**
* **Enable EIST Ambient Temp Overrule**
* **Typical Operating Speed 62 MPH**
* **MX Retarder State Cruise Control On (Manual Mode Engine Parameter)**
* **Powertrain Optimized for Balance**
* **EPA Emission Warranty**
* **3 PACCAR Premium 12V Starting Batteries 3000 CCA**
* **Belt Driven Variable Speed Fan Clutch MX-11/MX-13**
* **Exhaust Single RH Side of Cab DPF/SCR right-hand Under Cab.**
* **18" Ht, 5" Dia Chrome, Clear Coat Curved Tip Standpipe(s)**
* **Muffler Guard/Fairing Stainless Steel Half Round**
* **Eaton Fuller 10 Speed Transmission**
* **RPL20 Driveline lnteraxle**
* **RPL25 SD Driveline, 1 Midship Bearing**
* **Differential Lock and Interaxle lock**
* **Pull Cords All Air Tanks**
* **Horizontal AE Mounting Bar Double Spring**
* **Omit Trailer Hand Valve**
* **12' AE Lines Coiled, (2) 7-Way Plugs BOC/BOS socket AE Connections Without Hose Tenna**
* **FF: BR 14ply 295/75R22.5 R268 Ecopia HR 225**
* **FF: Accu-Lite Steel Armor 51487PK 22.5X8.25 PHP10-5 hand holes.**
* **26" Aluminum 100 Gallon Fuel Tank LH BOC Paddle handle filler cap with threadless filler neck**
* **Location LH BOC 100 Gallon**
* **DEF To Fuel Ratio 2:1 Or Greater**
* **RH Tank None Furnished**
* **LH Sleeper Baggage Door**
* **RH Painted Sleeper Vent**
* **LH Sleeper Side Tilting Window**
* **Aero Rear View Mirror Housing - Body Color**
* **Body Color – School Bus Yellow**
* **ConcertClass, AM/FM, Weatherband, 3.5 Aux**
* **Two Speaker Package For Cab**
* **Two Speaker Package For Sleeper**
* **Radio Mute When In Reverse**
* **Bluetooth Phone and Audio**
* **USB Port**
* **CB Terminal Wiring, Microphone Clip, Speaker F /0 CB radio mounted center of header.**
* **One Antenna for Factory Installed or F/O CB Mounted LH cowl, low mount only, with antenna cable.**
* **Triangle Reflector Kit**
* **Fire Extinguisher, Mounted Outboard Driver Seat Hazmat approval UL listed/rated ABC**
* **Increased Air Filter Full Indication**
* **Trailer Reservoir Air Pressure**
* **Main Instrumentation Panel**
* **Digital Cluster 15" Display with Speedometer, Tachometer, Primary Air Pressure, Secondary Air Pressure, Fuel Level, DEF Level, DPF Filter Status, Fuel Economy, Oil Pressure, Coolant Temp, and Voltmeter.**
* **Sleeper Digital Alarm Clock**
* **Two Load Lights, Incandescent, Flush mount Low lnbd Back of cab / back of sleeper**
* **Fuel Price Index Factor $507 NET**
* **44in Sleeper/ Prestige Interior {3M)**

\*\* Note here any exceptions taken to specifications/options listed above: