**Specifications**

1. All chemicals and treatments must be in compliance with Louisiana Structural Pest Control Law, Rules and Regulations for termite control work in Louisiana as adopted by the Pest Control Operators Association and approved by the Structural Pest Control Commission.
2. Contractor must be licensed with the Department of Agriculture and the Department of Entomology and should submit a copy of the license with the bid.
3. Contractor will be required to have on hand or immediately available an adequate supply of termite control materials to meet the agency’s needs.

Termite Baiting System Specifications

* The Termite Baiting Systems active ingredient must be registered by the Department of Agriculture and Forestry.
* Tamper resistant bait containers must be used to limit access to authorized personnel only.

Bait Station Replacement and Inspection

* Bait Station placement should be done in accordance with label directions and manufacturer’s recommendations. Spacing should be at industry standard intervals around the entire perimeter of the building. Walkways, driveways, parking areas and other cement or asphalt covering adjacent to the structure will be cored or capped with tamper resistant covers.
* All stations must be inspected according to label directions and manufacturer recommendations or state law, whichever is more stringent. When termites are detected in a monitoring device, one or more additional stations will be installed within 6 to 12 inches of the infested device if feasible.

 Record Keeping and Documentation

* An updated status report will be provided after each monitoring and/or baiting.
* Copies of these reports will be retained on file at the PCO contractor’s place of business.