**Scope of work:**

Contractor shall provide all labor and materials to furnish and install approximately one thousand three hundred feet (1300’) of chain link fence, six feet (6’) tall with three (3) strands of barbed wire on top at the John Franks WMA for the Louisiana Department of Wildlife and Fisheries.

**Location:**

John Franks WMA

HWY 3049

Shreveport, LA 71107

**Specifications:**

* Contractor shall install approximately one thousand three hundred feet (1300’) of chain link fence around the future site of the John Franks WMA head quarters.
* Installed fence shall be six feet (6’) tall with three (3) strands of barbed wire on top.
* Installed fence shall have:
  + Three inch (3”) corner, pull and gate posts
  + Two inch (2”) line posts on ten foot (10’) center
  + One and 5/8 inch (1 5/8”) top rail
  + Seven gauge (7ga) tension wire at bottom
  + Nine gauge (9ga) galvanized steel chain link fence fabric
  + All pipes shall be schedule 40
  + Barbed wire shall not be lighter than twelve gauge (12ga), galvanized, double barbed with reverse twist
* Contractor shall install 2 (two) twenty foot (20’) wide double swing gates one (1) at the main entrance and 1 (one) on the west side of the compound.

**Terms and Conditions:**

* Contractor is responsible for all trash and waste disposal
* Work shall be 7:00 AM to 5:30 PM Monday through Friday unless approved by Seth Miller.
* Please contact Seth Miller at (318) 371-5225 or (318) 243-6194 to setup day and time for site inspection.